Boeing 777-200 (All Models)
---------------------------------------------------------------------
Boeing 777 - REFERENCE INFORMATION
---------------------------------------------------------------------
SPECIFICATIONS

Cockpit Crew............................... 2
Seating Capacity......................... 400 (2-class)
Length........................................ 209 ft 1 in (63.7 m)
Wingspan................................... 199 ft 11 in (60.9 m)
Height........................................ 60 ft 9 in (18.5 m)
Typical Empty Weight.................. 304,500 lb (152.2 tons)
MTOW (Max Take-off Weight)...... 656,000 lb (328 tons)
Take-off Run at MTOW................ 11,600 ft
Max. Cruising Speed.................... Mach 0.84 at FL350
Service Ceiling ........................... 43,100 ft
Range........................................ 7,700 nm, 8,861 miles
======================================
ROLE

The Boeing 777 is a long-range, wide-body twin-engine jet
airliner. It is the world's largest twinjet and is commonly referred
to as the "Triple Seven". The aircraft has seating for over 300
passengers and has a range from 5,235 to 9,380 nm depending on
model. Its distinguishing features include the largest diameter
turbofan engines of any aircraft, six wheels on each main landing gear,
a circular fuselage cross-section and blade-shaped tail cone.
Developed in consultation with eight major airlines, the 777 was
designed to replace older wide-body airliners and bridge the capacity
difference between the 747 and 767.
First Flight............................... 12 June 1994
Number Produced of Type......... 855 as of March 2010 (in production)
Unit Cost................................. 777-200ER: $205 to 231 million
777-200LR: $237 to 263 million
777-300ER: $257 to 286 million
777-F: $252 to 260 million